City Hall District

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface fastethernet0/0

Router(config-if)#ip address 10.10.0.1 255.255.240.0

Router(config-if)#no shutdown

East End

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface fastethernet0/0

Router(config-if)#ip address 10.10.16.1 255.255.248.0

Router(config-if)#no shutdown

Crime Alley

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface fastethernet0/0

Router(config-if)#ip address 10.10.24.1 255.255.252.0

Router(config-if)#no shutdown

Diamond District

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface fastethernet0/0

Router(config-if)#ip address 10.10.28.1 255.255.254.0

Router(config-if)#no shutdown

Arkham Island

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface fastethernet0/0

Router(config-if)#ip address 10.10.30.1 255.255.254.0

Router(config-if)#no shutdown

Financial District

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface fastethernet0/0

Router(config-if)#ip address 10.10.34.1 255.255.254.0

Router(config-if)#no shutdown

City Hall District

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface serial0/0/0

Router(config-if)#ip address 10.10.32.42 255.255.255.248

Router(config-if)#no shutdown

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface serial0/0/0

Router(config-if)#ip address 10.10.32.34 255.255.255.248

Router(config-if)#no shutdown

East End

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface serial0/0/0

Router(config-if)#ip address 10.10.32.25 255.255.255.248

Router(config-if)#no shutdown

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface serial0/0/1

Router(config-if)#ip address 10.10.32.33 255.255.255.248

Router(config-if)#no shutdown

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface serial0/0/0

Router(config-if)#ip address 10.10.32.10 255.255.255.252

Router(config-if)#no shutdown

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface serial0/0/0

Router(config-if)#ip address 10.10.32.18 255.255.255.248

Router(config-if)#no shutdown

Crime Alley

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface serial0/0/0

Router(config-if)#ip address 10.10.32.2 255.255.255.248

Router(config-if)#no shutdown

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface serial0/0/0

Router(config-if)#ip address 10.10.32.9 255.255.255.248

Router(config-if)#no shutdown

Diamond District

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface serial0/0/0

Router(config-if)#ip address 10.10.32.1 255.255.255.248

Router(config-if)#no shutdown

Arkham Island

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface serial0/0/0

Router(config-if)#ip address 10.10.32.26 255.255.254.248

Router(config-if)#no shutdown

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface serial0/0/1

Router(config-if)#ip address 10.10.32.41 255.255.254.248

Router(config-if)#no shutdown

Financial District

Router>en

Router#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#interface serial0/1/0

Router(config-if)#ip address 10.10.32.17 255.255.255.248

Router(config-if)#no shutdown

Static route

Arkham Island

Router(config)#ip route 10.10.16.0 255.255.255.248 serial0/0/0

Router(config)#ip route 10.10.0.0 255.255.255.240 serial0/0/0

City Hall District

Router(config)#ip route 10.10.30.0 255.255.255.254 serial0/0/1

Router(config)#ip route 10.10.16.0 255.255.255.248 serial0/0/1

East End

Router(config)#ip route 10.10.0.0 255.255.255.240 serial0/0/1

Router(config)#ip route 10.10.30.0 255.255.255.254 serial0/0/0

Dynamic route

Financial District

Router>en

Router #config t

Enter configuration commands, one per line. End with CNTL/Z.

Router(config)#router rip

Router(config-router)#version 2

Router (config-router)#no auto-summary

Router (config-router)#network 10.10.32.16

Router (config-router)#passive-interface Fa0/0

Router (config-router)#exit

Crime Alley

Router >en

Router #config t

Enter configuration commands, one per line. End with CNTL/Z.

Router (config)#router rip

Router (config-router)#version 2

Router (config-router)#no auto-summary

Router (config-router)#network 10.10.32.8

Router (config-router)#network 10.10.32.0

Router (config-router)#passive-interface Fa0/0

Router (config-router)#exit

Diamond District

Router>en

Route r#config t

Enter configuration commands, one per line. End with CNTL/Z.

Router (config)#router rip

Router (config-router)#version 2

Router (config-router)#no auto-summary

Router (config-router)#network 10.10.28.0

Router (config-router)#passive-interface Fa0/0

Router (config-router)#exit